# Web Serial Port Connection Demo (Spectrometer)

This program is used to send spectrometer configuration commands and receive 16-bit (high-byte first) binary data streams for real-time plotting.

Spectrometer Status: Not Supported

### Serial Port Connection Settings

Baud Rate
Select Serial Device / Refresh

### Spectrometer Scanning Parameters

Integration Time (ms)
Start Wavelength (nm)
End Wavelength (nm)
Wavelength Interval (nm)

### Command Operations

Send Custom Command (e.g., version query):

## Spectrum Plot

## Serial Communication Log (Debug Info)